Plastic Coupling LC-APC Duplex green, ceramic sleeve

Plastic Coupling LC-APC Duplex green, ceramic sleeve,

LC-Duplex couplings in coloured plastic housing, which fit into SC-Simplex cut-outs. The couplings can be fixed with clips, also with sheet metal or threaded screws, which are available as accessories.

Connector type Connection 1: LC-Duplex

Connector type Connection 2: LC duplex

Design: SC-Simplex

Dust protection flap: Yes

Accessories: sheet metal screw

Housing material: plastic

Type of mounting: screw/engagement

Sleeve material: Ceramic

length: 29,2 mm

width: 22 mm

height: 9,3 mm

Operating temperature: -25°C - 70°C

Storage temperature: -40°C - 80°C

Conforms to standard: IEC 61754-20

Category: OS2

Colour: green

Suitable for fiber type: Singlemode

Version: LC / APC

Insertion loss 1310nmd: < 0.3 dB

Make: EFB-Elektronik GmbH

Item no.: 53343.31