Outdoor pipe socket, for branching and connecting, shrink version

Outdoor pipe socket, for branching and connecting, shrink version,

Green pipe socket with 3 cable entries for branching or connecting fibre optic cables. The sleeve is delivered with 2 splice holders. It is suitable for mast mounting as well as for underground installation. The seals are made of thermoplastic elastomer and Sconablend.

Suitable for number of fibres: 24

Splice Holder: Shrink

Number of splice holders: 2

Inputs/outputs: 3

Screw connections: M16

Protection class (IP): IP68

Cable diameter: 3.5 - 10.7 mm

Bending diameter fibre carrier: 42 mm

Max. Fibre storage length: 180 mm

Material: plastic

Colour: green

splice cassette: integrated

Can be buried: Yes

Tensile stress/compression: 55 N

Total length of the sleeve housing: 307 mm

Diameter of housing: 69 mm

Temperature range: -40°C - 70°C

Make: EFB-Elektronik GmbH

Item no.: 83189.1