FTTx compact connection box, connection: 2x SC-Simplex/LC-Duplex

FTTx compact connection box, connection: 2x SC-Simplex/LC-Duplex,

FTTx compact connection box with hinged fibre overlength cassette containing a splice protection receptacle. There are cut-outs for two cable entries in the box, as well as cut-outs for two flangeless SC-Simplex or LC-Duplex couplings.

Application: Indoor

Mounting type: Wall mounting

Possibility of mast mounting: No

Material: plastic

Colour: White

Maximum number of fibres: 4

Splice protection type: Shrinkage

Coupling type: SC Simplex/LC Duplex/E2000®

Max. Equipment (adapter): 2

IP Protection class: IP20

Protection against foreign bodies and accidental contact: Protection against medium-sized foreign bodies

Water protection: No protection

Dimensions: hxbxt 100mm x 80mm x 22mm

Temperature range: -20°C - 60°C

Access protection: Without

Make: EFB-Elektronik GmbH

Item no.: 53700.2