MDIC LSZH 4x9/125 white G.657A1 FTTH, singlemode, 3.7 mm, 750m Box

MDIC LSZH 4x9/125 white G.657A1 FTTH, singlemode, 3.7 mm, 750m box,

Micro Drop installation cable with outstanding mechanical properties. Due to G657.A1 fibers small bending radii are possible. Two support elements ensure stability and protection of the internal fibres. A two-sided tear seam facilitates stripping for quick installation. Particularly suitable for in-house applications at the line termination point (APL).

Application: Outside

Metal-free cable: Yes

Fiber type: Singlemode

Fibre category: G657A2

Fibre marking: Colour

Jacket material: LSZH

Coat colour: white

Flame retardant: according to EN 60332-1-2

Halogen-free: according to EN 50267-2-2

Low smoke: according to EN 61034-2

Temperature range (operation): -30°C - 70°C

Temperature range (storage): -30°C - 70°C

Temperature range (installation): -10°C - 50°C

Attenuation max.(dB/km) 1310nm: 0.35 dB/km

Attenuation max. (dB/km) 1550nm: 0.22 dB/km

Cabling standards: EN 50173-1; ISO/IEC 11801

Transmission standards: IEEE 802.3 10Mbit to 100Gbit

VDE designation: I-V(B)H 04E9/125

Structure: 4 x Singlemode G657.A1

Cable Ø: 3,7 mm

Weight: 16 kg/km

Bending radius: 37 mm

Tensile force Installation: 150 N

Make: EFB-Elektronik GmbH

Item no.: 56204.4