19" rack 84TE/3HE plus 1HE overlength cable compartment

19" 84TE/3HE subrack plus 1HE overlength cable compartment,

unassembled 19"/3HE subracks for 84HP with an additionally integrated 1HU overlength cable compartment, which can be pulled out to the rear/front. The total height is 4U. The 4U aluminium side panels are used for mounting in 19" devices. The subrack offers an 84TE depth-adjustable module carrier with 1TE pitch (1TE=5.08mm) and a front-mounted cable chamber panel with 5 cable brackets.

Included in delivery: 1 x subrack mounted, 1 x PG16 cable gland incl. locknut, 5 x cable brackets

Material: aluminium

Surface finish: powder-coated

Housing type: open

Ventilation openings available: Yes

Protection class (IP): IP20

width: 483 mm

height: 177,8 mm

Depth: 295 mm

Spacing (TE): 84 TE

Max. Modules: 12

Colour: aluminium/metal

Make: EFB-Elektronik GmbH

Item no.: 53711.1